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FAKRA Female Connector with Cable Assembly (A Coding to Z Coding)
Product Description
FAKRA (Automated Expert Group) to establish a unified connector system and standards that everyone will follow. Due to its special standard locking system, FAKRA connectors meet the high performance and safety requirements of today's automotive industry.[image: ][image: ][image: ]



· General Information of Cable Assembly                                                   
Feature/Speed
-Primary and secondary locking systems for increased assembly security
-13 mechanical and colored coding with one neutral coding, refer to FAKRA coding on next page
-20 Gbps of data speed for the connected vehicle, supporting any modern radar, camera, lidar or sensor applications
Rated Current
1A Max
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-40℃ ~+105℃
Poles
1,2,4 Poles are available（Refer to SKU table）
Cable
RG 174, RTK 031, RG59, RG179, RG58/62 etc. (50, 61,75, 93,120 Ohm) options
Rentention Force Latch
≥ 110 N
Rentention Force Lock
≥80N (Primary)
≥60N (Secondary)
Compliant to Standard
Per ISO20860-1 and -2, USCAR17 and 18
Water Resistance Level
No/IPX7/IPX9K in locked condition options
Application
Driving modules, Camera, Antenna, GPS, Gateway/Switch modules, 4K displays, High-speed cable networking, Sensor-device connectivity, surround view cameras, 
Infotainment devices




  
· Dimensions of Related Components (Unit is mm)                                                        [image: ]
[image: ]


· General Information of Connector                                                         
Frequency Range:              DC-6GHz               Insulation Resistance:   1000MΩ min.        
Working Voltage:               335V max.             Impedance:     50 Ω Max.                 
Center Contact Resistance:        20mΩ max.           Return Loss:     ≥ 18 dB      
Dielectric Withstanding Voltage:   1000V min.            IP Rating:     No/IPX7/IPX9K in locked condition (options)
Temperature Range:            -40 °C to +105 °C        Housing/Center contact: PBT, PA/CuZn, CuBe, CuSn     
V.S.W.R(电压驻波比):           1.3 Max.               Mating Endurance:      ≥25 Cycles            
High Data Rates:                Up to 8Gbps  
[image: ]
[image: ][image: ]

· SKU Table                                                                              
SKU No.
Poles
Conn. Type
Type
Remark
T-FAKRASTF-01-Coding A-Z
1
Female
Straight
Coding A-Z
T-FAKRASTF-02-D8-Coding A-Z
2
Female
Straight
Double 8mm type, Coding A-Z
T-FAKRASTF-02-D12.7-Coding A-Z
2
Female
Straight
Double 12.7mm type, Coding A-Z
T-FAKRASTF-04-Coding A-Z
4
Female
Straight
Coding A-Z

Notes: Coding A-Z color
A Black
B White
C Blue
D Bordeaux violet
E Green
F Brown
G Grey
H Violet
I Beige
K Curry
L Carmin red
M Pastel orange
N Pastel green
Z Water blue



















FAKRA Male Connector Cable Assembly, (A Coding to Z Coding)
Product Description
FAKRA (Automated Expert Group) to establish a unified connector system and standards that everyone will follow. Due to its special standard locking system, FAKRA connectors meet the high performance and safety requirements of today's automotive industry.
                       
[image: ][image: ][image: ]







· General Information of Cable Assembly                                                   
Feature/Speed
-Primary and secondary locking systems for increased assembly security
-13 mechanical and colored coding with one neutral coding, refer to FAKRA coding on next page
-20 Gbps of data speed for the connected vehicle, supporting any modern radar, camera, lidar or sensor applications
Rated Current
1A Max
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-40℃ ~+105℃
Poles
1,2 Poles are available（Refer to SKU table）
Cable
RG 174, RTK 031, RG59, RG179, RG58/62 etc. (50, 61,75, 93,120 Ohm) options
Rentention Force Latch
≥ 110 N
Rentention Force Lock
≥80N (Primary)
≥60N (Secondary)
Compliant to Standard
Per ISO20860-1 and -2, USCAR17 and 18
Water Resistance Level
No/IPX7/IPX9K in locked condition options
Application
Driving modules, Camera, Antenna, GPS, Gateway/Switch modules, 4K displays, High-speed cable networking, Sensor-device connectivity, surround view cameras, 
Infotainment devices



· Dimensions of Related Components (Unit is mm)                                                        [image: ]
[image: ]

· General Information of Connector                                                         
Frequency Range:               DC-6GHz                  Insulation Resistance:   1000MΩ min.        
Working Voltage:               335V max.                Impedance:     50 Ω Max.                 
Center Contact Resistance:        20mΩ max.              Return Loss:     ≥ 18 dB      
Dielectric Withstanding Voltage:   1000V min.               IP Rating:     IPX7/IPX9K in locked condition (options)
Temperature Range:            -40 °C to +105 °C           Housing/Center contact: PBT, PA/CuZn, CuBe, CuSn     
V.S.W.R(电压驻波比):           1.3 Max.                 Mating Endurance:      ≥25 Cycles            
High Data Rates: Up to 8Gbps 
[image: ]
[image: ]




· SKU Table                                                                              
SKU No.
Poles
Conn. Type
Type
Remark
T-FAKRASTM-01-Coding A-Z
1
Male
Straight
Coding A-Z
T-FAKRASTM-02-D8-Coding A-Z
2
Male
Straight
Double 8mm type, Coding A-Z
T-FAKRASTM-02-D12.7-Coding A-Z
2
Male
Straight
Double 12.7mm type, Coding A-Z

Notes: Coding A-Z color
A Black
B White
C Blue
D Bordeaux violet
E Green
F Brown
G Grey
H Violet
I Beige
K Curry
L Carmin red
M Pastel orange
N Pastel green
Z Water blue



















MINI FAKRA Female Connector with Cable Assembly
Product Description
The High-Speed FAKRA Mini Coaxial Cable Solution delivers 20 Gbps of data speed for the connected vehicle, reducing installation space requirements by up to 80 percent compared to traditional FAKRA, supporting any modern radar, camera, lidar or sensor applications.[image: ][image: ]



· General Information of Cable Assembly                                                   
Feature/Speed
-Primary and secondary locking systems for increased assembly security
-Multiple color-coded enclosures provide visual guidance during assembly and prevent connectors from mismatching with different keyway options. 
-20 Gbps of data speed for the connected vehicle, supporting any modern radar, camera, lidar or sensor applications
Rated Current
1A Max
Rated Voltage
60V AC/DC
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-40℃ ~+105℃
Poles
1,2,4 Poles are available（Refer to SKU table）
Cable
RG 174, RTK 031, RTK044 etc. (50/75 Ohm) options
Rentention Force Latch
≥ 110 N
Rentention Force Lock
≥80N (Primary)
≥60N (Secondary)


  
· Dimensions of Related Components (Unit is mm)                                                        [image: ]



· General Information of Connector                                                         
Frequency Range:               DC-15GHz              Insulation Resistance:   1000MΩ min.              
Working Voltage:               335V max.              Impedance:            50 Ω Max.                
Center Contact Resistance:        15mΩ max.             High Data Rates:       Up to 8Gbps               
Dielectric Withstanding Voltage:   1000V min.             Mating Endurance:      ≥25 Cycles                      
Temperature Range:            -40 °C to +105 °C          Housing/Center contact: PBT-GF                   
Return Loss:  ≥ 25 dB@DC-3GHz, (≥ -20db@3-6GHz, ≥ -12db@6-9GHz)
[image: ][image: ]
[image: ]

· SKU Table                                                                              
SKU No.
Poles
Conn. Type
Type
Remark
T-MFAKRASTF-01-Coding A-Z
1
Female
Straight
Coding A-Z
T-MFAKRASTF-02-Coding A-Z
2
Female
Straight
Coding A-Z
T-MFAKRASTF-04-Coding A-Z
4
Female
Straight
Coding A-Z

Notes: Coding A-Z color
A Black
B White
C Blue
D Bordeaux violet
E Green
F Brown
G Grey
H Violet
I Beige
K Curry
L Carmin red
M Pastel orange
N Pastel green
Z Water blue




















Energy Storage: 2+12 Pin Molded Cable Assembly, Straight                            
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· Dimensions of Cable Assembly (Unit is mm)                                                           
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· General Information of Cable Assembly                                                   
Rated Current
100A 
Insulation Resistance
≥100MΩ
Operation Temperature
-40℃ ~+80℃
Poles
2+12 Pin （Refer to below SKU table）
Water Resistance Level
IP30 in locked condition
Cable
UL2517 2*5AWG+10*22AWG VW-1/FT1, PVC cable 
Temperature Rise Test
120A current lasted for 4H, temperature rise<50K (5AWG/17mm)











· SKU Table                                                                              
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-ESSTF-14-001
2+12
Female
Straight



· Dimensions of Mating Connector (Unit is mm)                                                       [image: ]





· General Information of Connector                                                         

Ambient Temperature:   -40℃ ~ +80℃                  Insulation Resistance:   ≥100MΩ                
Connector Body:        PA66+GF/94V-0                  Insert/Pull Force:       <100N                 
Connector Contacts:     Brass with silver plated            IP Rating:             IP30 in locked condition    
Compression Strength:   DC500V, leakage current <5mA     Mating Endurance:      3000 Cycles             

Solar Energy/Photovoltaic: MC4 Female Cable Assembly, Straight                            
[image: ][image: ]

















· Dimensions of Cable Assembly (Unit is mm)                                                          
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· General Information of Cable Assembly                                                   
Rated Current
30A 
Insulation Resistance
≥100MΩ
Contact Resistance
<0.35mΩ
Operation Temperature
-40℃ ~+80℃
Poles
1 Pin （Refer to below SKU table）
Water Resistance Level
IP67/IP68 in locked condition, optional
Cable
16-20AWG VW-1/FT1, PVT or customized 













· SKU Table                                                                              
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-MC4STF-01-001
1
Female
Straight



· Dimensions of Related Connector (Unit is mm)                                                       [image: ]





· General Information of Connector                                                         

Ambient Temperature:   -40℃ ~ +80℃                  Insulation Resistance:   ≥100MΩ                
Connector Body:        PA66+GF/94V-0                  Insert/Pull Force:       <100N                 
Connector Contacts:     Brass with silver plated            IP Rating:       IP67/IP68 in locked condition optional
Rated Current/Voltage:   30A/1000V                  

Solar Energy/Photovoltaic: MC4 Male Cable Assembly, Straight                            
[image: ][image: ]
















· Dimensions of Cable Assembly (Unit is mm)                                                          
[image: ]














· General Information of Cable Assembly                                                   
Rated Current
30A 
Insulation Resistance
≥100MΩ
Contact Resistance
<0.35mΩ
Operation Temperature
-40℃ ~+80℃
Poles
1 Pin （Refer to below SKU table）
Water Resistance Level
IP67/IP68 in locked condition, optional
Cable
16-20AWG VW-1/FT1, PVT or customized 












· SKU Table                                                                              
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-MC4STF-01-001
1
Male
Straight



· Dimensions of Related Connector (Unit is mm)                                                       [image: ]





· General Information of Connector                                                         

Ambient Temperature:   -40℃ ~ +80℃                  Insulation Resistance:   ≥100MΩ                
Connector Body:        PA66+GF/94V-0                  Insert/Pull Force:       <100N                 
Connector Contacts:     Brass with silver plated            IP Rating:       IP67/IP68 in locked condition optional
Rated Current/Voltage:   30A/1000V                  







M23 Male Charging/Discharging Battery Connector, Molded Cable Assembly                         
[image: ][image: ]

















· Dimensions of Cable Assembly (Unit is mm)                                                          
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· General Information of Cable Assembly                                                   
Rated Current
[bookmark: OLE_LINK2]50A/10A/3A 
Rated Voltage
500V/300V/60V /DC
Insulation Resistance
≥100MΩ
Contact Resistance
≤10 mΩ
Operation Temperature
-40℃ ~+105℃
Poles
2+0, 2+5, 2+1+3, 2+1+5 Pins Optional (Refer to below SKU table and pin picture）, straight or right angle optional
Water Resistance Level
IP67/IP68 in locked condition, optional
Cable
8AWG*2C+16AWG*1C+22AWG*5C,PVC or customized













· Difference Pins as Below:                                                                  
[image: ]· SKU Table                                                                              
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-EM23STM-2-001
2+0
Male
Straight

T-EM23STM-7-001
2+5
Male
Straight

T-EM23STM-6-001
2+1+3
Male
Straight

T-EM23STM-8-001
2+1+5
Male
Straight

T-EM23RAM-2-001
2+0
Male
[bookmark: OLE_LINK3]Right Angle

T-EM23RAM-7-001
2+5
Male
Right Angle

T-EM23RAM-6-001
2+1+3
Male
Right Angle

T-EM23RAM-8-001
2+1+5
Male
Right Angle





· Dimensions of Related Connector (Unit is mm)                                                       [image: ]


· General Information of Connector                                                         

Ambient Temperature:   -40℃ ~ +105℃                 Insulation Resistance:   ≥100MΩ                  
Connector Body:        UL94V-0                        Rated Current:       20-50A                     
Connector Contacts:     Brass with silver/golded plated    IP Rating:    IP67/IP68 in locked condition optional
M23 Male With Base, Charging/Discharging Battery Connector, Cable Assembly                         

[image: ][image: ]










· General Information of Cable Assembly                                                   
Rated Current
50A/10A/3A 
Rated Voltage
500V/300V/60V /DC
Insulation Resistance
≥100MΩ
Contact Resistance
≤10 mΩ
Operation Temperature
-40℃ ~+105℃
Poles
2+1+5 Pins is available (Refer to below SKU table), 2+0, 2+5, 2+1+3 PIN can be customized
Water Resistance Level
IP67/IP68 in locked condition, optional
Cable
8AWG*2C+16AWG*1C+22AWG*5C,PVC or customized













· SKU Table                                                                              
SKU No.
Poles
Conn. Type
Type
Remark
T-EM23BM-2-001
2+0
Male
Assembly

T-EM23BM-7-001
2+5
Male
Assembly

T-EM23BM-6-001
2+1+3
Male
Assembly

T-EM23BM-8-001
2+1+5
Male
Assembly






· Dimensions of Related Connector (Unit is mm)                                                  
[image: ]






· General Information of Connector                                                         

Ambient Temperature:   -40℃ ~ +105℃                 Insulation Resistance:   ≥100MΩ                  
Connector Body:        UL94V-0                        Rated Current:       20-50A                     
Connector Contacts:     Brass with silver/golded plated    IP Rating:    IP67/IP68 in locked condition optional












M23 Female Charging/Discharging Battery Connector, Cable Assembly                         
[image: ][image: ]











· General Information of Cable Assembly                                                   
Rated Current
50A/10A/3A 
Rated Voltage
500V/300V/60V /DC
Insulation Resistance
≥100MΩ
Contact Resistance
≤10 mΩ
Operation Temperature
-40℃ ~+105℃
Poles
2+0, 2+5, 2+1+3, 2+1+5 Pins Optional (Refer to below SKU table and pin picture）
Water Resistance Level
IP67/IP68 in locked condition, optional
Cable
8AWG*2C+16AWG*1C+22AWG*5C,PVC or customized












· Difference Pins as Below:                                                                  
[image: ]
· SKU Table                                                                              
SKU No.
Poles
Conn. Type
Type
Remark
T-EM23BF-2-001
2+0
Female
Assembly

T-EM23BF-7-001
2+5
Female
Assembly

T-EM23BF-6-001
2+1+3
Female
Assembly

T-EM23BF-8-001
2+1+5
Female
Assembly




· Dimensions of Related Connector (Unit is mm)                                                       [image: ]


· General Information of Connector                                                         

Ambient Temperature:   -40℃ ~ +105℃                 Insulation Resistance:   ≥100MΩ                  
Connector Body:        UL94V-0                        Rated Current:       20-50A                     
Connector Contacts:     Brass with silver/golden plated      IP Rating:    IP67/IP20/IP68 in locked condition optional





















[bookmark: OLE_LINK4]Customized, Type C, Female Cable Assembly, IP68                         
[image: ][image: ]















· Dimensions of Cable Assembly (Unit is mm)                                                          · General Information of Cable Assembly                                                   
Rated Voltage
30V /DC
Insulation Resistance
≥5MΩ
Contact Resistance
≤3Ω
Water Resistance Level
IP68 in locked condition
Cable
UL2464 22AWG*4C PVC blk, can be customized

[image: ]

· SKU Table                                                                              
SKU No.
Poles
Conn. Type
Type
Remark
T-CUSTC4F-002
4
Female
Assembly
Customized



· Dimensions of Related Connector (Unit is mm)                                             
[image: ]






· General Information of Connector                                                         

Ambient Temperature:   -25℃ ~ +85℃                  Insulation Resistance:   ≥5MΩ                  
Connector Body:        PBT, black                      Fire resistance：        UL94V-0            
Connector Contacts:     Brass with silver/golden plated   





Customized, 4Pin Male Cable Assembly For Smart System, IP67                         
[image: ][image: ]















· Dimensions of Cable Assembly (Unit is mm)                                                     [image: ]




· General Information of Cable Assembly                                                   
Rated Voltage
12V /DC
Insulation Resistance
≥10MΩ
Contact Resistance
≤3Ω
Water Resistance Level
IP67 in locked condition
Cable
Cable, length can be customized
Application
· Original Bosch replacement cable, Connects the drive unit with the control unit


· SKU Table                                                                              
SKU No.
Poles
Conn. Type
Overmold Type
Remark
T-CUS4M-002
4
Male
Straight
Customized



· Dimensions of Related Connector (Unit is mm)                                             
[image: ]






· General Information of Connector                                                         

Ambient Temperature:   -20℃ ~ +80℃                  Insulation Resistance:   ≥100MΩ                  
Connector Body:        PA66, black                     Fire resistance：       UL94V-0                 
Connector Contacts:     Brass with golden plated          Water Resistance:      IP66                     





Customized, 4Pin Female Cable Assembly For Smart System, IP67                         
[image: ][image: ]















· Dimensions of Cable Assembly (Unit is mm)                                                   [image: ]


· General Information of Cable Assembly                                                   
Rated Voltage
12V /DC
Insulation Resistance
≥10MΩ
Contact Resistance
≤3Ω
Water Resistance Level
IP67 in locked condition
Cable
Cable, length can be customized
Application
· Original Bosch replacement cable, Connects the drive unit with the control unit



· SKU Table                                                                              
SKU No.
Poles
Conn. Type
Overmold Type
Remark
T-CUS4F-002
4
Female
Straight
Customized



· Dimensions of Related Connector (Unit is mm)                                             
[image: ]






· General Information of Connector                                                         

Ambient Temperature:   -20℃ ~ +80℃                  Insulation Resistance:   ≥100MΩ                  
Connector Body:        PA66, black                     Fire resistance：       UL94V-0                
Connector Contacts:     Brass with golden plated           Water Resistance:      IP66                   vel





CPC 9PIN Female Molded Cable Assembly                           [image: ][image: ]













· Dimensions of Cable Assembly (Unit is mm)                                                          
[image: ]









· General Information of Cable Assembly                                                    
Rated Current
13A Max.(Series1); 7.5A Max.(Series2); 25A Max.(Series3); 
25A Max.(Series4); 50A Max.(Series5); 50A Max.(Series6);
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
8,17 Poles are available,
3,4,5,12 can be customized （Refer to below SKU table）
Water Resistance Level
IP67, IP68 can be customized (In locked condition)
Cable
PUR/PVC cable options
















· [image: ]Shape A and Shape B of Locked Key （Optional）                                          

· Pinouts（Optional for difference CNC connector）
[image: ]· SKU Table                                                                              
Assembly SKU No.
Connector Information
Cable Assembly

Poles
Conn. Type
Locked Key
Series
Shell Size
Overmoding or Assembly Type
T-CPCS1STF-5-04-001-Shell 11
4
Female
5
1
11
Customized
T-CPCS1STF-4-04-001-Shell 11
4
Female
4
1
11
Customized
T-CPCS1STF-5-09-001-Shell 13
9
Female
5
1
13
      Optional
T-CPCS1STF-4-09-001-Shell 13
9
Female
4
1
13
Optional
T-CPCS1STF-5-14-001-Shell 17
14
Female
5
1
17
Customized
T-CPCS1STF-4-14-001-Shell 17
14
Female
4
1
17
Customized
T-CPCS1STF-5-16-001-Shell 17
16
Female
5
1
17
Customized
T-CPCS1STF-4-16-001-Shell 17
16
Female
4
1
17
Customized
T-CPCS1STF-5-24-001-Shell 23
24
Female
5
1
23
Customized
T-CPCS1STF-4-24-001-Shell 23
24
Female
4
1
23
Customized
T-CPCS1STF-5-37-001-Shell 23
37
Female
5
1
23
Customized
T-CPCS1STF-4-37-001-Shell 23
37
Female
4
1
23
Customized




	Assembly SKU No.
	Connector Information
	Cable Assembly

	
	Poles
	Conn. Type
	Locked Key
	Series
	Shell Size
	Overmoding or Assembly Type

	T-CPCS2STF-5-08-001-Shell 11
	8
	Female
	5
	2
	11
	Customized

	T-CPCS2STF-4-08-001-Shell 11
	8
	Female
	4
	2
	11
	Customized

	T-CPCS2STF-5-09-001-Shell 11
	9
	Female
	5
	2
	11
	      Optional

	T-CPCS2STF-4-09-001-Shell 11
	9
	Female
	4
	2
	11
	Optional

	T-CPCS2STF-5-28-001-Shell 17
	28
	Female
	5
	2
	17
	Customized

	T-CPCS2STF-4-28-001-Shell 17
	28
	Female
	4
	2
	17
	Customized

	T-CPCS2STF-5-57-001-Shell 23
	57
	Female
	5
	2
	23
	Customized

	T-CPCS2STF-4-57-001-Shell 23
	57
	Female
	4
	2
	23
	Customized

	T-CPCS2STF-5-63-001-Shell 23
	63
	Female
	5
	2
	23
	Customized

	T-CPCS2STF-4-63-001-Shell 23
	63
	Female
	4
	2
	23
	Customized

	T-CPCS3STF-5-3-001-Shell 17
	3
	Female
	5
	3
	17
	Customized

	T-CPCS3STF-4-3-001-Shell 17
	3
	Female
	4
	3
	17
	Customized

	T-CPCS3STF-5-7-001-Shell 23
	7
	Female
	5
	3
	23
	Customized

	T-CPCS3STF-4-7-001-Shell 23
	7
	Female
	4
	3
	23
	Customized

	T-CPCS4STF-5-13-001-Shell 23
	13
	Female
	5
	4
	23
	Customized

	T-CPCS4STF-4-13-001-Shell 23
	13
	Female
	4
	4
	23
	Customized

	T-CPCS4STF-5-16-001-Shell 23
	16
	Female
	5
	4
	23
	Customized

	T-CPCS4STF-4-16-001-Shell 23
	16
	Female
	4
	4
	23
	Customized

	T-CPCS4STF-5-22-001-Shell 23
	22
	Female
	5
	4
	23
	Customized

	T-CPCS4STF-4-22-001-Shell 23
	22
	Female
	4
	4
	23
	Customized

	T-CPCS5STF-5-3-001-Shell 17
	3
	Female
	5
	5
	17
	Customized

	T-CPCS5STF-4-3-001-Shell 17
	3
	Female
	4
	5
	17
	Customized

	T-CPCS6STF-5-16-001-Shell 23
	16
	Female
	5
	6
	23
	Customized

	T-CPCS6STF-4-16-001-Shell 23
	16
	Female
	4
	6
	23
	Customized



· Dimensions of Related Components (Unit is inch)                                          [image: ]

· General Information of Connector                                                         

Ambient Temperature:   -55℃ ~ +105℃                 Insulation Resistance:   ≥100MΩ                
Connector Body:        Glass filled nylon 6/6,black         IP Rating:             IP65,IP67 optional                 
Connector Contacts:     Brass with gold plated         
· CPC Series Information of Connector                                                   
Items
Description
Contact Shape
Series 1
Standard, Terminal OD with 1.57mm, 13A Max, 4-37P
[image: ]
Series 2
High Density, Terminal OD with 1.02mm, 7.5A Max, 8-63P
[image: ]
Series 3
Power Density, 25A Max., 13P, 16P, 22P
[image: ]
Series 4
Power and Signal combine, Signal 13A max.; Power 25A Max., 13P, 16P, 22P
[image: ]
Series 5
Power Density (Seal IP65/67 optional), Power with 50A Max., with 3x Powerband
[image: ]
Series 6
Power and Signal combine (Seal optional), Signal 13A max., Power 50A Max., with 2x powerband and 8x III+ signal contact
[image: ]



CPC 9PIN Male Molded Cable Assembly                           [image: ][image: ]














· Dimensions of Cable Assembly (Unit is mm)                                                           

[image: ]











· General Information of Cable Assembly                                                    
Rated Current
13A Max.(Series1); 7.5A Max.(Series2); 25A Max.(Series3); 
25A Max.(Series4); 50A Max.(Series5); 50A Max.(Series6);
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
8,17 Poles are available,
3,4,5,12 can be customized （Refer to below SKU table）
Water Resistance Level
IP67, IP68 can be customized ( in locked condition)
Cable
PUR/PVC cable options















· [image: ]Shape A and Shape B of Locked Key （Optional）                                           

· Pinouts（Optional for difference CNC connector）
[image: ]· SKU Table                                                                              
Assembly SKU No.
Connector Information
Cable Assembly

Poles
Conn. Type
Locked Key
Series
Shell Size
Overmoding or Assembly Type
T-CPCS1STM-5-04-001-Shell 11
4
Male
5
1
11
Customized
T-CPCS1STM-4-04-001-Shell 11
4
Male
4
1
11
Customized
T-CPCS1STM-5-09-001-Shell 13
9
Male
5
1
13
      Optional
T-CPCS1STM-4-09-001-Shell 13
9
Male
4
1
13
Optional
T-CPCS1STM-5-14-001-Shell 17
14
Male
5
1
17
Customized
T-CPCS1STM-4-14-001-Shell 17
14
Male
4
1
17
Customized
T-CPCS1STM-5-16-001-Shell 17
16
Male
5
1
17
Customized
T-CPCS1STM-4-16-001-Shell 17
16
Male
4
1
17
Customized
T-CPCS1STM-5-24-001-Shell 23
24
Male
5
1
23
Customized
T-CPCS1STM-4-24-001-Shell 23
24
Male
4
1
23
Customized
T-CPCS1STM-5-37-001-Shell 23
37
Male
5
1
23
Customized
T-CPCS1STM-4-37-001-Shell 23
37
Male
4
1
23
Customized



	Assembly SKU No.
	Connector Information
	Cable Assembly

	
	Poles
	Conn. Type
	Locked Key
	Series
	Shell Size
	Overmoding or Assembly Type

	T-CPCS2STM-5-08-001-Shell 11
	8
	Male
	5
	2
	11
	Customized

	T-CPCS2STM-4-08-001-Shell 11
	8
	Male
	4
	2
	11
	Customized

	T-CPCS2STM-5-09-001-Shell 11
	9
	Male
	5
	2
	11
	      Optional

	T-CPCS2STM-4-09-001-Shell 11
	9
	Male
	4
	2
	11
	Optional

	T-CPCS2STM-5-28-001-Shell 17
	28
	Male
	5
	2
	17
	Customized

	T-CPCS2STM-4-28-001-Shell 17
	28
	Male
	4
	2
	17
	Customized

	T-CPCS2STM-5-57-001-Shell 23
	57
	Male
	5
	2
	23
	Customized

	T-CPCS2STM-4-57-001-Shell 23
	57
	Male
	4
	2
	23
	Customized

	T-CPCS2STM-5-63-001-Shell 23
	63
	Male
	5
	2
	23
	Customized

	T-CPCS2STM-4-63-001-Shell 23
	63
	Male
	4
	2
	23
	Customized

	T-CPCS3STM-5-3-001-Shell 17
	3
	Male
	5
	3
	17
	Customized

	T-CPCS3STM-4-3-001-Shell 17
	3
	Male
	4
	3
	17
	Customized

	T-CPCS3STM-5-7-001-Shell 23
	7
	Male
	5
	3
	23
	Customized

	T-CPCS3STM-4-7-001-Shell 23
	7
	Male
	4
	3
	23
	Customized

	T-CPCS4STM-5-13-001-Shell 23
	13
	Male
	5
	4
	23
	Customized

	T-CPCS4STM-4-13-001-Shell 23
	13
	Male
	4
	4
	23
	Customized

	T-CPCS4STM-5-16-001-Shell 23
	16
	Male
	5
	4
	23
	Customized

	T-CPCS4STM-4-16-001-Shell 23
	16
	Male
	4
	4
	23
	Customized

	T-CPCS4STM-5-22-001-Shell 23
	22
	Male
	5
	4
	23
	Customized

	T-CPCS4STM-4-22-001-Shell 23
	22
	Male
	4
	4
	23
	Customized

	T-CPCS5STM-5-3-001-Shell 17
	3
	Male
	5
	5
	17
	Customized

	T-CPCS5STM-4-3-001-Shell 17
	3
	Male
	4
	5
	17
	Customized

	T-CPCS6STM-5-16-001-Shell 23
	16
	Male
	5
	6
	23
	Customized

	T-CPCS6STM-4-16-001-Shell 23
	16
	Male
	4
	6
	23
	Customized



· Dimensions of Related Components (Unit is mm/inch)                                          [image: ]

· General Information of Connector                                                         

Ambient Temperature:   -55℃ ~ +105℃                 Insulation Resistance:   ≥100MΩ                
Connector Body:        Glass filled nylon 6/6,black         IP Rating:             IP65,IP67 optional                 
Connector Contacts:     Brass with gold plated         
· CPC Series Information of Connector                                                   
Items
Description
Contact Shape
Series 1
Standard, Terminal OD with 1.57mm, 13A Max, 4-37P
[image: ]
Series 2
High Density, Terminal OD with 1.02mm, 7.5A Max, 8-63P
[image: ]
Series 3
Power Density, 25A Max., 13P, 16P, 22P
[image: ]
Series 4
Power and Signal combine, Signal 13A max.; Power 25A Max., 13P, 16P, 22P
[image: ]
Series 5
Power Density (Seal IP65/67 optional), Power with 50A Max., with 3x Powerband
[image: ]
Series 6
Power and Signal combine (Seal optional), Signal 13A max., Power 50A Max., with 2x powerband and 8x III+ signal contact
[image: ]


· SKU Table                                                                               
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-M12ASTM-03-001
3
Male
Straight
With Metal Nut/Screw thread
T-M12ASTM-04-001
4
Male
Straight
With Metal Nut/Screw thread
T-M12ASTM-05-001
5
Male
Straight
With Metal Nut/Screw thread
T-M12ASTM-08-001
8
Male
Straight
With Metal Nut/Screw thread
T-M12ASTM-12-001
12
Male
Straight
With Metal Nut/Screw thread
T-M12ASTM-17-001
17
Male
Straight
With Metal Nut/Screw thread



[bookmark: OLE_LINK5]M12 Female (A Coding) Molded Cable, Straight, With Metal Nut (Screw Thread)                            [image: ][image: ]













· Dimensions of Cable Assembly (Unit is mm)                                                          
[image: ]










· General Information of Cable Assembly                                                   
Rated Current
2A Max (6-8Pins), 4A Max (2-5Pins), 1.5A Max. (9-17Pins) 
Rated Voltage
30/60V DC
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
4, 8,12 Poles are available, 
3,5,17 can be customized （Refer to below SKU table）
Water Resistance Level
IP67, IP68 in locked condition
Cable
PUR/PVC cable (22-28AWG) options











· Pins Layout                                                                              

[image: ]


· SKU Table                                                                              
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-M12ASTF-03-001
3
Female
Straight
With Metal Nut/Screw thread
T-M12ASTF-04-001
4
Female
Straight
With Metal Nut/Screw thread
T-M12ASTF-05-001
5
Female
Straight
With Metal Nut/Screw thread
T-M12ASTF-08-001
8
Female
Straight
With Metal Nut/Screw thread
T-M12ASTF-12-001
12
Female
Straight
With Metal Nut/Screw thread
T-M12ASTF-17-001
17
Female
Straight
With Metal Nut/Screw thread



· Dimensions of Related Components  (Unit is mm)                                                       [image: ]



· General Information of Connector                                                         

Ambient Temperature:   -20℃ ~ +80℃                 Insulation Resistance:   ≥100MΩ                
Connector Body:        PA66                         Contact Resistance:     ≤10mΩ                 
Connector Contacts:     Brass with gold plated            Shield:               Available                
Coupling Nut/Screw:     Zinc alloy with nickel plated       IP Rating:             IP67,IP68 in locked condition
Seal/O-ring:            Silicone                       Mating Endurance:      >500 Cycles             



M12 Male (A Coding) Molded Cable, Straight, With Metal Nut (Screw Thread)                            [image: ][image: ]














· Dimensions of Cable Assembly  (Unit is mm)                                                           


[image: ]










· General Information of Cable Assembly                                                    
Rated Current
2A Max (6-8Pins), 4A Max (2-5Pins), 1.5A Max. (9-17Pins) 
Rated Voltage
30/60V DC
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
8,17 Poles are available,
3,4,5,12 can be customized （Refer to below SKU table）
Water Resistance Level
IP67, IP68 in locked condition
Cable
PUR/PVC cable (22-28AWG) options
















· Pins Layout                                                                              

[image: ]

· SKU Table                                                                               
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-M12ASTM-03-001
3
Male
Straight
With Metal Nut/Screw thread
T-M12ASTM-04-001
4
Male
Straight
With Metal Nut/Screw thread
T-M12ASTM-05-001
5
Male
Straight
With Metal Nut/Screw thread
T-M12ASTM-08-001
8
Male
Straight
With Metal Nut/Screw thread
T-M12ASTM-12-001
12
Male
Straight
With Metal Nut/Screw thread
T-M12ASTM-17-001
17
Male
Straight
With Metal Nut/Screw thread



· The Dimensions of Related Components (Unit is mm)                                                  [image: ]


· General Information of Connector                                                           
Ambient Temperature:  -20℃ ~ +80℃                   Insulation Resistance:   ≥100MΩ                    
Connector Body:       PA66                           Contact Resistance:     ≤10mΩ                     
Connector Contacts:    Brass with gold plated             Shield:                Available                   
Coupling Nut/Screw:    Zinc alloy with nickel plated        IP Rating:              IP67,IP68 in locked condition   
Mating Endurance:     >500 Cycles         


M12 Female (A Coding) Molded Cable, Right Angle, With Metal Nut (Screw Thread)                            [image: ][image: ]
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· Dimensions of Cable Assembly (Unit is mm)                                                           


[image: ]













· General Information of Cable Assembly                                                    
Rated Current
2A Max (6-8Pins), 4A Max (2-5Pins), 1.5A Max. (9-17Pins) 
Rated Voltage
30/60V DC
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
5,8 Poles are available,
3,4,12,17 can be customized （Refer to below SKU table）
Water Resistance Level
IP67, IP68 in locked condition
Cable
PUR/PVC cable (22-28AWG) options













· Pins Layout                                                                             

[image: ]

· SKU Table                                                                              
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-M12ARAF-03-001
3
Female
Right Angle
With Metal Nut/Screw thread
T-M12ARAF-04-001
4
Female
Right Angle
With Metal Nut/Screw thread
T-M12ARAF-05-001
5
Female
Right Angle
With Metal Nut/Screw thread
T-M12ARAF-08-001
8
Female
Right Angle
With Metal Nut/Screw thread
T-M12ARAF-12-001
12
Female
Right Angle
With Metal Nut/Screw thread
T-M12ARAF-17-001
17
Female
Right Angle
With Metal Nut/Screw thread



· Dimensions of Related Components (Unit is mm)                                                       [image: ]

· General Information of Connector                                                         

Ambient Temperature:   -20℃ ~ +80℃                   Insulation Resistance:    ≥100MΩ                 
Connector Body:        PA66                           Contact Resistance:      ≤10mΩ                  
Connector Contacts:     Brass with gold plated              Shield:                Available                 
Coupling Nut/Screw:     Zinc alloy with nickel plated         IP Rating:              IP67,IP68 in locked condition 
Seal/O-ring:            Silicone                         Mating Endurance:      >500 Cycles               



M12 Male (A Coding) Molded Cable, Right Angle, With Metal Nut (Screw Thread)                            [image: ][image: ]
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· Dimensions of Cable Assembly (Unit is mm)                                                           
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· General Information of Cable Assembly                                                     
Rated Current
2A Max (6-8Pins), 4A Max (2-5Pins), 1.5A Max. (9-17Pins) 
Rated Voltage
30/60V DC
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
3,4,5,8,12,17 can be customized （Refer to below SKU table）
Water Resistance Level
IP67, IP68 in locked condition
Cable
PUR/PVC cable (22-28AWG) options












· Pins Layout                                                                             

[image: ]

· SKU Table                                                                             
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-M12ARAM-03-001
3
Male
Right Angle
With Metal Nut/Screw thread
T-M12ARAM-04-001
4
Male
Right Angle
With Metal Nut/Screw thread
T-M12ARAM-05-001
5
Male
Right Angle
With Metal Nut/Screw thread
T-M12ARAM-08-001
8
Male
Right Angle
With Metal Nut/Screw thread
T-M12ARAM-12-001
12
Male
Right Angle
With Metal Nut/Screw thread
T-M12ARAM-17-001
17
Male
Right Angle
With Metal Nut/Screw thread


· Dimensions of Related Components (Unit is mm)                                                      [image: ]


· General Information of Connector                                                           

Ambient Temperature:   -20℃ ~ +80℃                   Insulation Resistance:   ≥100MΩ                  
Connector Body:        PA66                           Contact Resistance:     ≤10mΩ                   
Connector Contacts:     Brass with gold plated             Shield:                Available                  
Coupling Nut/Screw:     Zinc alloy with nickel plated        IP Rating:             IP67,IP68 in locked condition  
Mating Endurance:      >500 Cycles             


M12 Male (D Coding) Molded Cable, Straight, With Metal Nut (Screw Thread)                            [image: ] [image: ]
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· Dimensions of Cable Assembly (Unit is mm)                                                           


[image: ]












· General Information of Cable Assembly                                                     
Rated Current
4A Max.
Rated Voltage
30V/60V DC
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
4 Poles straight are available, right angle can be customized (refer to SKU Table)
Water Resistance Level
IP67 in locked condition, IP68 Can be customized
Cable
PUR/PVC cable (18-24AWG) options

· SKU Table                                                                                
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-M12DSTM-04-001
4
Male
Straight
With Metal Nut/Screw thread
T-M12DRAM-04-001
4
Male
Right angle
With Metal Nut/Screw thread




· Dimensions of Related Components (Unit is mm)                                                       
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· General Information of Connector                                                         

Ambient Temperature:   -25℃ ~ +80℃                   Insulation Resistance:   ≥100MΩ                
Connector Body:        PA66                           Contact Resistance:     ≤10mΩ                 
Connector Contacts:     Brass with gold plated              Shield:               Available                
Coupling Nut/Screw:    Zinc alloy with nickel plated          IP Rating:             IP67 in locked condition    
Mating Endurance:     >500 Cycles              















M12 Female (D Coding) Molded Cable, Straight, With Metal Nut (Screw Thread)                            [image: ][image: ] [image: ]
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· Dimensions of Cable Assembly (Unit is mm)                                                           


[image: ]











· SKU Table                                                                               
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-M12DSTF-04-001
4
Female
Straight
With Metal Nut/Screw thread
T-M12DRAF-04-001
4
Female
Right angle
With Metal Nut/Screw thread

· General Information of Cable Assembly                                                     
Rated Current
4A Max.
Rated Voltage
30V/60V DC
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
4 Poles straight are available, right angle can be customized (refer to SKU Table)
Water Resistance Level
IP67 in locked condition, IP68 Can be customized
Cable
PUR/PVC cable (18-24AWG) options














· Dimensions of Related Components (Unit is mm)                                                       


[image: ]















· General Information of Connector                                                         

Ambient Temperature:   -25℃ ~ +80℃                  Insulation Resistance:    ≥100MΩ                 
Connector Body:        PA66                          Contact Resistance:      ≤10mΩ                  
Connector Contacts:     Brass with gold plated             Shield:                Available                
Coupling Nut/Screw:     Zinc alloy with nickel plated        IP Rating:              IP67 in locked condition    
Mating Endurance:      >500 Cycles        






















	M12 Male (X Coding) Molded Cable, Straight, With Metal Nut (Screw Thread)                            
 [image: ][image: ]
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· Dimensions of Cable Assembly (Unit is mm)                                                         
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· General Information of Cable Assembly                                                     
Rated Current
0.5A Max.
Rated Voltage
48V DC
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-25℃ ~+85℃
Poles
8 Poles straight are available, right angle can be customized (refer to SKU Table)
Water Resistance Level
IP67 in locked condition, IP68 Can be customized
Cable
PUR/PVC cable (24, 26AWG) options






















· SKU Table                                                                                
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-M12XSTM-08-001
8
Male
Straight
With Metal Nut/Screw thread
T-M12XRAM-08-001
8
Male
Right angle
With Metal Nut/Screw thread





· Dimensions of Related Components (Unit is mm)                                                    
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· General Information of Connector                                                       
Ambient Temperature:   -25℃ ~ +85℃                  Insulation Resistance:  ≥100MΩ                
Connector Body:        PA66                          Contact Resistance:    ≤5mΩ                  
Connector Contacts:     Brass with gold plated             Shield:              Available                
Coupling Nut/Screw:     Zinc alloy with nickel plated        IP Rating:            IP67 in locked condition   
Mating Endurance:      >500 Cycles        












M8 Female (A Coding) Molded Cable, Straight, With Metal Nut (Screw Thread) [image: ][image: ]
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· Dimensions of Cable Assembly (Unit is mm)                                                          
[image: ]













· General Information of Cable Assembly                                                   
Rated Current
1.5A Max (6-8Pins), 3A Max (3-5Pins)
Rated Voltage
30/60V DC
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
3,4,6 Poles straight are available, 
5,8 straight can be customized （Refer to below SKU table）
3,4,5,6,8 right angle can be customized too （Refer to below SKU table）
Water Resistance Level
IP67, IP68 in locked condition
Cable
PUR/PVC cable (24-26AWG) options

























· Pins Layout                                                                           
[image: ]







· SKU Table                                                                             
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-M8ASTF-03-001
3
Female
Straight
With Metal Nut/Screw thread
T-M8ASTF-04-001
4
Female
Straight
With Metal Nut/Screw thread
T-M8ASTF-05-001
5
Female
Straight
With Metal Nut/Screw thread
T-M8ASTF-06-001
6
Female
Straight
With Metal Nut/Screw thread
T-M8ASTF-08-001
8
Female
Straight
With Metal Nut/Screw thread
T-M8ARAF-03-001
3
Female
Right Angle
With Metal Nut/Screw thread
T-M8ARAF-04-001
4
Female
Right Angle
With Metal Nut/Screw thread
T-M8ARAF-05-001
5
Female
Right Angle
With Metal Nut/Screw thread
T-M8ARAF-06-001
6
Female
Right Angle
With Metal Nut/Screw thread
T-M8ARAF-08-001
8
Female
Right Angle
With Metal Nut/Screw thread
















· Dimensions of Related Components (Unit is mm)                                                    
[image: ]




· General Information of Connector                                                      

Ambient Temperature:   -25℃ ~ +85℃                  Insulation Resistance:    ≥100MΩ               
Connector Body:        PA66                          Contact Resistance:      ≤5mΩ                 
Connector Contacts:     Brass with gold plated             Shield:                Available              
Coupling Nut/Screw:     Zinc alloy with nickel plated        IP Rating:              IP67 in locked condition  
Mating Endurance:      >500 Cycles                
M8 Male (A Coding) Molded Cable, Straight, With Metal Nut (Screw Thread)                             [image: ][image: ]
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· General Information of Cable Assembly                                                     
Rated Current
1.5A Max (6-8Pins), 3A Max (3-5Pins)
Rated Voltage
30/60V DC
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
3,4,6 Poles straight are available, 
5,8 straight can be customized （Refer to below SKU table）
3,4,5,6,8 right angle can be customized too （Refer to below SKU table）
Water Resistance Level
IP67 in locked condition
Cable
PUR/PVC cable (24-26AWG) options

























· SKU Table                                                                               
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-M8ASTM-03-001
3
Male
Straight
With Metal Nut/Screw thread
T-M8ASTM-04-001
4
Male
Straight
With Metal Nut/Screw thread
T-M8ASTM-05-001
5
Male
Straight
With Metal Nut/Screw thread
T-M8ASTM-06-001
6
Male
Straight
With Metal Nut/Screw thread
T-M8ASTM-08-001
8
Male
Straight
With Metal Nut/Screw thread
T-M8ARAM-03-001
3
Male
Right Angle
With Metal Nut/Screw thread
T-M8ARAM-04-001
4
Male
Right Angle
With Metal Nut/Screw thread
T-M8ARAM-05-001
5
Male
Right Angle
With Metal Nut/Screw thread
T-M8ARAM-06-001
6
Male
Right Angle
With Metal Nut/Screw thread
T-M8ARAM-08-001
8
Male
Right Angle
With Metal Nut/Screw thread









· Pins Layout                                                                           






· Dimensions of Cable Assembly (Unit is mm)                                                          
[image: ]













· Dimensions of Components                                                            
[image: ]




	

	· General Information of Connector                                                      

Ambient Temperature:   -25℃ ~ +85℃                  Insulation Resistance:    ≥100MΩ               
Connector Body:        PA66                          Contact Resistance:      ≤5mΩ                 
Connector Contacts:     Brass with gold plated             Shield:                Available              
Coupling Nut/Screw:     Zinc alloy with nickel plated        IP Rating:              IP67 in locked condition  
Mating Endurance:      >500 Cycles              

	



DIN Circle Female Molded Cable, Straight, With Shell 
[image: ][image: ]







· Dimensions of Cable Assembly (Unit is mm)                                                          
[image: ]










· General Information of Cable Assembly                                                      
Rated Current
2A Max.
Rated Voltage
12V DC
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
8 Poles straight are available, 
3-8 Poles straight can be customized （Refer to below SKU table）
Design Standard
Per VDE DIN standard
Cable
PUR/PVC cable (22-28AWG) options


· Pins Layout                                                                           
[image: ]

· SKU Table                                                                               
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-DINSTF-03-001
3
Female
Straight
With shell
T- DINSTF-04-001
4
Female
Straight
With shell
T- DINSTF-05-001
5
Female
Straight
With shell, Pins 180 degree
T- DINSTF-05-002
5
Female
Straight
With shell, one pin in the middle
T- DINSTF-06-001
6
Female
Straight
With shell
T- DINSTF-07-001
7
Female
Straight
With shell
T- DINSTF-08-001
8
Female
Straight
With shell



· Dimensions of Related Components (Unit is mm)                                                       
Connector
[image: ]













· General Information of Connector                                                         

Ambient Temperature:   -20℃ ~ +80℃                   Insulation Resistance:   ≥100MΩ                
Connector Body:        PBT+GF/ABS                     Contact Resistance:     ≤10mΩ                 
Connector Contacts:     Brass with silver/tin               Shell:                 Steel with nickel          Mating Endurance:      5000 Cycles                      Pull Force:             3.5+/1 kg               
DIN Circle Male Molded Cable, Straight, With Shell                             [image: ] [image: ]
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· Dimensions of Cable Assembly (Unit is mm)                                                            
[image: ]












· General Information of Cable Assembly                                                     
Rated Current
2A Max.
Rated Voltage
12V DC
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
8 Poles straight are available, 
3-8 Poles straight can be customized （Refer to below SKU table）
Design Standard
Per VDE DIN standard
Cable
PUR/PVC cable (22-28AWG) options


· Pins Layout                                                                             
[image: ]
· SKU Table                                                                               
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-DINSTM-03-001
3
Male
Straight
With shell
T- DINSTM-04-001
4
Male
Straight
With shell
T- DINSTM-05-001
5
Male
Straight
With shell, Pins with 180 degree
T- DINSTM-05-002
5
Male
Straight
With shell, Pins within 240 degree
T- DINSTM-06-001
6
Male
Straight
With shell
T- DINSTM-07-001
7
Male
Straight
With shell
T- DINSTM-08-001
8
Male
Straight
With shell




· Dimensions of Related Components (Unit is mm)                                                       

Connector 
[image: ]














· General Information of Connector                                                         

Ambient Temperature:   -20℃ ~ +80℃                   Insulation Resistance:   ≥100MΩ                 
Connector Body:        PBT+GF/ABS                     Contact Resistance:     ≤10mΩ                  
Connector Contacts:     Brass with silver/tin               Shell:                 Steel with nickel           Mating Endurance:      5000 Cycles                      Pull Force:             3.5+/1 kg                


DIN Male Molded Cable, Right Angle, With Shell                             [image: ][image: ]












· Dimensions of Cable Assembly (Unit is mm)                                                            
[image: ]




















· General Information of Cable Assembly                                                     
Rated Current
2A Max.
Rated Voltage
12V DC
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
8 Poles straight are available, 
3-8 Poles straight can be customized （Refer to below SKU table）
Design Standard
Per VDE DIN standard
Cable
PUR/PVC cable (22-28AWG) options


· Pins Layout                                                                            
[image: ]
· SKU Table                                                                               
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-DINRAM-03-001
3
Male
Right Angle
With shell
T- DINRAM-04-001
4
Male
Right Angle
With shell
T- DINRAM-05-001
5
Male
Right Angle
With shell, Pins with 180 degree
T- DINRAM-05-002
5
Male
Right Angle
With shell, Pins within 240 degree
T- DINRAM-06-001
6
Male
Right Angle
With shell
T- DINRAM-07-001
7
Male
Right Angle
With shell
T- DINRAM-08-001
8
Male
Right Angle
With shell



· Dimensions of Related Components (Unit is mm)                                                        
Connector 
[image: ]
















· General Information of Connector                                                          
Ambient Temperature:   -20℃ ~ +85℃                   Insulation Resistance:   ≥100MΩ                 
Connector Body:        PBT+GF/ABS                     Contact Resistance:     ≤10mΩ                  
Connector Contacts:     Brass with silver/tin               Shell:                 Steel with nickel           Mating Endurance:      5000 Cycles                      Pull Force:             3.5+/1 kg                


9Pin MINI DIN Female Molded Cable, Straight, With Shell 
[image: ] [image: ]


















· Dimensions of Cable Assembly (Unit is mm)                                                           
[image: ]








· General Information of Cable Assembly                                                     
Rated Current
1.5A Max.
Rated Voltage
12V 
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
3-9 Poles straight can be customized（Refer to below SKU table）
Design Standard
Per VDE DIN standard
Cable
PUR/PVC cable (22-28AWG) options













· Pins Layout                                                                            
[image: ]


· SKU Table                                                                               
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-MDINSTF-03-001
3
Female
Straight
With shell
T- MDINSTF-04-001
4
Female
Straight
With shell
T- MDINSTF-05-001
5
Female
Straight
With shell
T- MDINSTF-06-001
6
Female
Straight
With shell
T- MDINSTF-07-001
7
Female
Straight
With shell
T- MDINSTF-08-001
8
Female
Straight
With shell
T- MDINSTF-09-001
9
Female
Straight
With shell



· Dimensions of Related Components (Unit is mm)                                                       
Connector
[image: ]














· General Information of Connector                                                           

Ambient Temperature:   -20℃ ~ +80℃                   Insulation Resistance:   ≥100MΩ                  
Connector Body:        PBT+GF/ABS                     Contact Resistance:     ≤10mΩ                   
Connector Contacts:     Brass with silver/tin               Shell:                 Steel with nickel           
MINI DIN Male Molded Cable, Straight, With Shell                              [image: ][image: ]















· Dimensions of Cable Assembly (Unit is mm)                                                           
[image: ]













· General Information of Cable Assembly                                                     
Rated Current
1.5A Max.
Rated Voltage
12V
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
6, 8 Poles are available, 3-9 Poles straight can be customized（Refer to SKU table）
Design Standard
Per VDE DIN standard
Cable
PUR/PVC cable (22-28AWG) options



· Pins Layout                                                                           
[image: ]

· SKU Table                                                                               
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-MDINSTM-03-001
3
Male
Straight
With shell
T- MDINSTM-04-001
4
Male
Straight
With shell
T- MDINSTM-05-001
5
Male
Straight
With shell
T- MDINSTM-06-001
6
Male
Straight
With shell
T- MDINSTM-07-001
7
Male
Straight
With shell
T- MDINSTM-08-001
8
Male
Straight
With shell
T- MDINSTM-09-001
9
Male
Straight
With shell



· Dimensions of Related Components (Unit is mm)                                                       
Connector 
[image: ]














· General Information of Connector                                                         

Ambient Temperature:   -20℃ ~ +80℃                   Insulation Resistance:   ≥100MΩ                 
Connector Body:        PBT+GF/ABS                     Contact Resistance:     ≤10mΩ                  
Connector Contacts:     Brass with silver/tin               Shell:                 Steel with nickel          




9Pin D-SUB Female Molded Cable Assembly, Straight 
 [image: ][image: ]







· Dimensions of Cable Assembly  (Unit is mm)                                                          
[image: ]











· General Information of Cable Assembly                                                      
Rated Current
4A Max.
Rated Voltage
30V
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+70℃
Poles
9 Poles straight are available, 
9 Poles right angle can be customized （Refer to below SKU table）
Cable
PUR/PVC cable (18-28AWG) options
Water Resistance
IP67 in lock condition can be customized if need














· SKU Table                                                                                   
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-DSUBSTF-09-001
9
Female
Straight
Locking type: Fix screw
T- DSUBRAF-09-001
9
Female
Right Angle
Locking type: Fix screw





· Dimensions of Related Components (Unit is mm)                                                       
Connector
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· General Information of Connector                                                           

Ambient Temperature:   -25℃ ~ +70℃                   Insulation Resistance:   ≥100MΩ                
Connector Body:        PBT                            Contact Resistance:     ≤10mΩ                 
Connector Contacts:     Brass with nickel/gold plated        Shell:                 Unavailable             
Pitch：                2.84mm                        Mating Endurance:      500 Cycles              


9 Pin D-SUB Male Molded Cable Assembly, Straight                               [image: ][image: ]















· Dimensions of Cable Assembly  (Unit is mm)                                                          
[image: ]















· SKU Table                                                                             
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-DSUBSTM-09-001
9
Male
Straight
Locking type: Fix screw
T- DSUBRAM-09-001
9
Male
Right Angle
Locking type: Fix screw

· General Information of Cable Assembly                                                   
Rated Current
4A Max.
Rated Voltage
30V
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+70℃
Poles
9 Poles straight are available, 
9 Poles right angle can be customized （Refer to below SKU table）
Cable
PUR/PVC cable (18-28AWG) options
Water Resistance
IP67 in lock condition can be customized if need



· Dimensions of Connector (Unit is mm)                                                               Connector 
[image: ]






· General Information of Connector                                                          

Ambient Temperature:   -25℃ ~ +70℃                   Insulation Resistance:   ≥100MΩ                
Connector Body:        PBT                            Contact Resistance:     ≤10mΩ                 
Connector Contacts:     Brass with nickel/gold plated        Shell:                 Unavailable             
Pitch：                2.84mm                        Mating Endurance:      500 Cycles              





15 Pin D-SUB Female Molded Cable Assembly, Straight [image: ] [image: ]








· Dimensions of Cable Assembly (Unit is mm)                                                          
[image: ]













· SKU Table                                                                               
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-DSUBSTF-15-001
15
Female
Straight
Locking type: Fix screw
T- DSUBRAF-15-001
15
Female
Right Angle
Locking type: Fix screw

· General Information of Cable Assembly (Unit is mm)                                                    
Rated Current
4A Max.
Rated Voltage
30V
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+70℃
Poles
15 Poles straight are available, 
15 Poles right angle can be customized （Refer to below SKU table）
Cable
PUR/PVC cable (18-28AWG) options
Water Resistance
IP67 in lock condition can be customized if need















· Dimensions of Connector (Unit is mm)                                                                
Connector
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· General Information of Connector                                                         

Ambient Temperature:   -25℃ ~ +70℃                   Insulation Resistance:   ≥100MΩ               
Connector Body:        PBT                            Contact Resistance:     ≤10mΩ                
Connector Contacts:     Brass with nickel/gold plated        Shell:                 Unavailable            
Pitch：                2.84mm                        Mating Endurance:      500 Cycles             





15 Pin D-SUB Male Molded Cable Assembly, Straight                             
  [image: ][image: ]















· Dimensions of Cable Assembly (Unit is mm)                                                           
[image: ]











· General Information of Cable Assembly                                                    
Rated Current
4A Max.
Rated Voltage
30V
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+70℃
Poles
15 Poles straight are available, 
15 Poles right angle can be customized （Refer to below SKU table）
Cable
PUR/PVC cable (18-28AWG) options
Water Resistance
IP67 in lock condition can be customized if need


· SKU Table                                                                                
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-DSUBSTM-15-001
15
Male
Straight
Locking type: Fix screw
T- DSUBRAM-15-001
15
Male
Right Angle
Locking type: Fix screw



· Dimensions of Connector (Unit is mm)                                                                 Connector 
[image: ]









· General Information of Connector                                                         

Ambient Temperature:   -25℃ ~ +70℃                   Insulation Resistance:   ≥100MΩ               
Connector Body:        PBT                            Contact Resistance:     ≤10mΩ                
Connector Contacts:     Brass with nickel/gold plated        Shell:                 Unavailable            
Pitch：                2.84mm                        Mating Endurance:      500 Cycles             




25 Pin D-SUB Female Molded Cable Assembly, Straight 
[image: ] [image: ]









· Dimensions of Cable Assembly (Unit is mm)                                                            
[image: ]














· SKU Table                                                                                  
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-DSUBSTF-25-001
25
Female
Straight
Locking type: Fix screw
T- DSUBRAF-25-001
25
Female
Right Angle
Locking type: Fix screw

· General Information of Cable Assembly                                                     
Rated Current
4A Max.
Rated Voltage
30V
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+70℃
Poles
25 Poles straight are available, 
25 Poles right angle can be customized （Refer to below SKU table）
Cable
PUR/PVC cable (18-28AWG) options
Water Resistance
IP67 in lock condition can be customized if need


· Dimensions of Connector (Unit is mm)                                                                  
Connector
[image: ]



















· General Information of Connector                                                          
Ambient Temperature:   -25℃ ~ +70℃                   Insulation Resistance:   ≥100MΩ               
Connector Body:        PBT                            Contact Resistance:     ≤10mΩ                
Connector Contacts:     Brass with nickel/gold plated        Shell:                 Unavailable            
Pitch：                2.84mm                        Mating Endurance:      500 Cycles             
25 Pin D-SUB Male Molded Cable Assembly, Straight                             [image: ]  [image: ]


















· Dimensions of Cable Assembly (Unit is mm)                                                            
[image: ]














· General Information of Cable Assembly                                                     
Rated Current
4A Max.
Rated Voltage
30V
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+70℃
Poles
25 Poles straight are available, 
25 Poles right angle can be customized （Refer to below SKU table）
Cable
PUR/PVC cable (18-28AWG) options
Water Resistance
IP67 in lock condition can be customized if need












· SKU Table                                                                               
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-DSUBSTM-25-001
25
Male
Straight
Locking type: Fix screw
T- DSUBRAM-25-001
25
Male
Right Angle
Locking type: Fix screw


· Dimensions of Connector (Unit is mm)                                                                 Connector 
[image: ]







· General Information of Connector                                                          
Ambient Temperature:   -25℃ ~ +70℃                   Insulation Resistance:   ≥100MΩ               
Connector Body:        PBT                            Contact Resistance:     ≤10mΩ                 
Connector Contacts:     Brass with nickel/gold plated        Shell:                 Unavailable             
Pitch：                2.84mm                        Mating Endurance:      500 Cycles              





37Pin D-SUB Female Molded Cable Assembly, Straight 
[image: ] [image: ] 










· Dimensions of Cable Assembly  (Unit is mm)                                                           
[image: ]

















· General Information of Cable Assembly                                                    
Rated Current
4A Max.
Rated Voltage
30V
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+70℃
Poles
37 Poles straight and right angle can be customized (Refer to below SKU table)
Cable
PUR/PVC cable (18-28AWG) options
Water Resistance
IP67 in lock condition can be customized if need

· SKU Table                                                                                
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-DSUBSTF-37-001
37
Female
Straight
Locking type: Fix screw
T- DSUBRAF-37-001
37
Female
Right Angle
Locking type: Fix screw


· Dimensions of Connector (Unit is mm)                                                                
Connector
[image: ]





















· General Information of Connector                                                          
Ambient Temperature:   -25℃ ~ +70℃                   Insulation Resistance:   ≥100MΩ               
Connector Body:        PBT                            Contact Resistance:     ≤10mΩ                
Connector Contacts:     Brass with nickel/gold plated        Shell:                Unavailable             
Pitch：                2.84mm                        Mating Endurance:     500 Cycles              




37 Pin D-SUB Male Molded Cable Assembly, Straight                          [image: ][image: ]

   











· Dimensions of Cable Assembly (Unit is mm)                                                           
[image: ]













· SKU Table                                                                                
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-DSUBSTM-37-001
37
Male
Straight
Locking type: Fix screw
T- DSUBRAM-37-001
37
Male
Right Angle
Locking type: Fix screw

· General Information of Cable Assembly                                                    
Rated Current
4A Max.
Rated Voltage
30V
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+70℃
Poles
37 Poles straight are available, 
37 Poles right angle can be customized （Refer to below SKU table）
Cable
PUR/PVC cable (18-28AWG) options
Water Resistance
IP67 in lock condition can be customized if need


· Dimensions of Connector (Unit is mm)                                                                Connector 
[image: ]






· General Information of Connector                                                          

Ambient Temperature:   -25℃ ~ +70℃                  Insulation Resistance:   ≥100MΩ                
Connector Body:        PBT                           Contact Resistance:     ≤10mΩ                 
Connector Contacts:     Brass with nickel/gold plated       Shell:                Unavailable              
Pitch：                2.84mm                       Mating Endurance:      500 Cycles              





15Pin High Density D-SUB Female Molded Cable Assembly, Straight  [image: ][image: ] 







· Dimensions of Cable Assembly (Unit is mm)                                                           
[image: ]





· SKU Table                                                                              
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-HDBSTF-15-001
15
Female
Straight
Locking type: Fix screw
T-HDBSTF-26-001
26
Female
Straight
Locking type: Fix screw
T-HDBSTF-44-001
44
Female
Straight
Locking type: Fix screw
T-HDBSTF-62-001
62
Female
Straight
Locking type: Fix screw
T-HDBSTF-78-001
78
Female
Straight
Locking type: Fix screw
T-HDBRAF-15-001
15
Female
Right Angle
Locking type: Fix screw
T-HDBRAF-26-001
26
Female
Right Angle
Locking type: Fix screw
T-HDBRAF-44-001
44
Female
Right Angle
Locking type: Fix screw
T-HDBRAF-62-001
62
Female
Right Angle
Locking type: Fix screw
T-HDBRAF-78-001
78
Female
Right Angle
Locking type: Fix screw

· General Information of Cable Assembly                                                   
Rated Current
5A Max.
Rated Voltage
30V
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+70℃
Poles
15 Poles straight is available,
26, 44,62,78 Poles straight/right angle can be customized (Refer to SKU table)
Cable
PUR/PVC cable (18-28AWG) options
Water Resistance
IP67 in lock condition can be customized if need


· Dimensions of Connector  (Unit is mm)                                                           Connector
[image: ]





· General Information of Connector                                                         

Ambient Temperature:   -25℃ ~ +70℃                  Insulation Resistance:   ≥100MΩ               
Connector Body:        PBT                            Contact Resistance:     ≤15mΩ                
Connector Contacts:     Brass with nickel/gold plated        Shell:                Unavailable             
Pitch：                1.98mm                        Mating Endurance:     500 Cycles              






15Pin High Density D-SUB Male Molded Cable Assembly, Straight                             [image: ][image: ]











· Dimensions of Cable Assembly (Unit is mm)                                                            
[image: ]









· SKU Table                                                                               
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-HDBSTM-15-001
15
Male
Straight
Locking type: Fix screw
T-HDBSTM-26-001
26
Male
Straight
Locking type: Fix screw
T-HDBSTM-44-001
44
Male
Straight
Locking type: Fix screw
T-HDBSTM-62-001
62
Male
Straight
Locking type: Fix screw
T-HDBSTM-78-001
78
Male
Straight
Locking type: Fix screw
T- HDBRAM-15-001
15
Male
Right Angle
Locking type: Fix screw
T- HDBRAM-26-001
26
Male
Right Angle
Locking type: Fix screw
T- HDBRAM-44-001
44
Male
Right Angle
Locking type: Fix screw
T- HDBRAM-62-001
62
Male
Right Angle
Locking type: Fix screw
T- HDBRAM-78-001
78
Male
Right Angle
Locking type: Fix screw

· General Information of Cable Assembly                                                    
Rated Current
5A Max.
Rated Voltage
30V
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+70℃
Poles
15 Poles straight are available, 
26, 44,62,78 Poles straight/right angle can be customized （Refer to SKU table）
Cable
PUR/PVC cable (18-28AWG) options
Water Resistance
IP67 in lock condition can be customized if need



· Dimensions of Connector (Unit is mm)                                                                
Connector
[image: ]


· General Information of Connector                                                          

Ambient Temperature:   -25℃ ~ +70℃                  Insulation Resistance:   ≥100MΩ                
Connector Body:        PBT                           Contact Resistance:     ≤15mΩ                 
Connector Contacts:     Brass with nickel/gold plated       Shell:                Unavailable              
Pitch：                1.98mm                       Mating Endurance:     500 Cycles               

27W2 Hybrid D-SUB Female Molded Cable Assembly, Straight 
[image: ] [image: ] 











· Dimensions of Cable Assembly (Unit is mm)                                                            


[image: ]














· General Information of Cable Assembly                                                    
Rated Current
7.5A Max.
Rated Voltage
30V
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
5W5,7W2, 9W4, 11W1, 13W3, 27W2 Poles straight/right angle can be customized (Refer to SKU table)
Cable
PUR/PVC cable (16-20AWG) options
Water Resistance
IP67 in lock condition can be customized if need






· Dimensions of Connector (Unit is mm)                                                                  Connector
[image: ]






· General Information of Connector                                                           

Ambient Temperature:   -25℃ ~ +70℃                   Insulation Resistance:   ≥100MΩ                
Connector Body:        PBT                            Contact Resistance:     ≤15mΩ                  
Connector Contacts:     Brass with nickel/gold plated        Shell:                Unavailable               
Pitch：                2.84mm                        Mating Endurance:     500 Cycles.               








27W2 Hybrid D-SUB Male Molded Cable Assembly, Straight                             
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· Dimensions of Cable Assembly (Unit is mm)                                                            

[image: ]













· General Information of Cable Assembly                                                     
Rated Current
7.5A Max.
Rated Voltage
30V
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
27W2 Poles straight are available, 
5W5,7W2, 9W4, 11W1, 13W3 Poles straight/right angle can be customized (Refer to SKU table) 
Cable
PUR/PVC cable (16-20AWG) options
Water Resistance
IP67 in lock condition can be customized if need


· SKU Table                                                                               
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-HDSUBSTM-05-001
5+0
Male
Straight
Locking type: Fix screw
T-HDSUBSTM-07-001
5+2
Male
Straight
Locking type: Fix screw
T-HDSUBSTM-09-001
5+4
Male
Straight
Locking type: Fix screw
T-HDSUBSTM-11-001
10+1
Male
Straight
Locking type: Fix screw
T-HDSUBSTM-13-001
10+3
Male
Straight
Locking type: Fix screw
T-HDSUBSTM-27-001
25+2
Male
Straight
Locking type: Fix screw
T-HDSUBRAM-05-001
5+0
Male
Right Angle
Locking type: Fix screw
T-HDSUBRAM-07-001
5+2
Male
Right Angle
Locking type: Fix screw
T-HDSUBRAM-09-001
5+4
Male
Right Angle
Locking type: Fix screw
T-HDSUBRAM-11-001
10+1
Male
Right Angle
Locking type: Fix screw
T-HDSUBRAM-13-001
10+3
Male
Right Angle
Locking type: Fix screw
T-HDSUBRAM-27-001
25+2
Male
Right Angle
Locking type: Fix screw


· Dimensions of Connector (Unit is mm)                                                                
Connector 
[image: ]



· General Information of Connector                                                          

Ambient Temperature:   -35℃ ~ +85℃                   Insulation Resistance:   ≥100MΩ               
Connector Body:        PBT                            Contact Resistance:     ≤15mΩ                
Connector Contacts:     Brass with nickel/gold plated        Shell:                Available               
Pitch：                2.84mm                        Mating Endurance:     500 Cycles              

9Pin Micro D-SUB Female Molded Cable Assembly, Straight 
[image: ] [image: ] 







· Dimensions of Cable Assembly (Unit is mm)                                                            

[image: ]










· SKU Table                                                                              
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-MDSUBSTF-09-001
9
Female
Straight

T-MDSUBRAF-09-001
9
Female
Right Angle

T-MDSUBSTF-15-001
15
Female
Straight

T-MDSUBRAF-15-001
15
Female
Right Angle

T-MDSUBSTF-25-001
25
Female
Straight

T-MDSUBRAF-25-001
25
Female
Right Angle


· General Information of Cable Assembly                                                   
Rated Current
1A Max.
Rated Voltage
30V
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
9, 15, 25 Poles straight/right angle can be customized (Refer to below SKU table)
Cable
PUR/PVC cable (26-28AWG) options
Water Resistance
IP67 in lock condition can be customized if need


· Dimensions of Connector (Unit is mm)                                                                  Connector
[image: ]






· General Information of Connector                                                         

Ambient Temperature:   -35℃ ~ +85℃                  Insulation Resistance:   ≥100MΩ                 
Connector Body:        PBT                           Contact Resistance:     45mΩ max.               
Connector Contacts:     Brass with nickel/gold plated       Shell:                 Available                
Pitch：                1.27mm                       Mating Endurance:      500 Cycles               







USB 2.0 Type A Female Molded Cable Assembly, Straight 
 [image: ][image: ] 









· Dimensions of Cable Assembly (Unit is mm)                                                 


[image: ]












· SKU Table                                                                               
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-USB2.0ASTF-04-001
4
Female
Straight


· General Information of Cable Assembly                                                    
Rated Current
1.5A Max.
Rated Voltage
30V
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
4 Poles straight is available, refer to below SKU table
Cable
USB2.0 24-28AWG cable ,PUR/PVC options


· Related Components (Unit is mm)                                                         Connector
[image: ]
[image: ]





· General Information of Connector                                                          
Ambient Temperature:   -20℃ ~ +80℃                     Insulation Resistance:    ≥100MΩ            
Connector Body:        PBT, BLK/WHT                      Contact Resistance:     30mΩ Max.          
Connector Contacts:     Copper Alloy with gold plated          Shell:                 Stainless steel       
Fire Resistance：       UL94V-0                           Insert Force:           35N max.           




USB 2.0 Type A Male Molded Cable Assembly, Straight                             
[image: ][image: ]















· Dimensions of Cable Assembly (Unit is mm)                                                 

[image: ]










· General Information of Cable Assembly                                                    
Rated Current
1.5A Max.
Rated Voltage
30V 
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
4 Poles straight is available, refer to below SKU table
Cable
USB2.0 24-28AWG cable ,PUR/PVC options

· SKU Table                                                                                
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-USB2.0ASTM-04-001
4
Male
Straight




· Dimensions of Connector (Unit is mm)                                                     
Connector 
[image: ]


[image: ]


· General Information of Connector                                                          

Ambient Temperature:   -20℃ ~ +80℃                      Insulation Resistance:   ≥100MΩ             
Connector Body:        PBT, BLK/WHT                       Contact Resistance:     30mΩ Max.          
Connector Contacts:     Phosphor Bronze with gold plated       Shell:                Stainless steel         
Fire Resistance：       UL94V-0                            Insert Force:           35N max.           




USB 2.0 Type A Male Molded Cable Assembly, Right Angle                             

[image: ][image: ]














· Dimensions of Cable Assembly (Unit is mm)                                                 

[image: ]










· General Information of Cable Assembly                                                    
Rated Current
1.5A Max.
Rated Voltage
30V
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
4 Poles is available, refer to below SKU table
Cable
USB2.0 24-28AWG cable, PUR/PVC options

· SKU Table                                                                                
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-USB2.0ARAM-04-001
4
Male
Right Angle




· Dimensions of Connector (Unit is mm)                                                     
Connector 
[image: ]
[image: ]


· General Information of Connector                                                          

Ambient Temperature:   -20℃ ~ +80℃                     Insulation Resistance:   ≥100MΩ             
Connector Body:        PBT, BLK/WHT                      Contact Resistance:     30mΩ Max.          
Connector Contacts:     Phosphor Bronze with gold plated       Shell:                Stainless steel         
Fire Resistance：       UL94V-0                           Insert Force:           35N max.           


USB 2.0 Type B Male Molded Cable Assembly, Straight                             

[image: ][image: ]














· Dimensions of Cable Assembly (Unit is mm)                                                            

[image: ]










· General Information of Cable Assembly                                                    
Rated Current
1.5A Max.
Rated Voltage
30V
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
4 Poles straight is available, refer to below SKU table
Cable
USB2.0 24-28AWG cable, PUR/PVC options

· SKU Table                                                                                
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-USB2.0BSTM-04-001
4
Male
Straight




· Dimensions of Connector (Unit is mm)                                                     
Connector 
[image: ]

[image: ]

· General Information of Connector                                                          

Ambient Temperature:   -20℃ ~ +80℃                      Insulation Resistance:   ≥100MΩ             
Connector Body:        PBT, BLK/WHT                       Contact Resistance:     30mΩ Max.          
Connector Contacts:     Phosphor Bronze with gold plated       Shell:                 Stainless steel         
Fire Resistance：        UL94V-0                           Insert Force:           35N max.           



USB 2.0 Type B Male Molded Cable Assembly, Right Angle                             

[image: ][image: ]














· Dimensions of Cable Assembly (Unit is mm)                                                            

[image: ]










· General Information of Cable Assembly                                                    
Rated Current
1.5A Max.
Rated Voltage
30V
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
4 Poles is available, refer to below SKU table
Cable
USB2.0 24-28AWG cable, PUR/PVC options

· SKU Table                                                                                
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-USB2.0BRAM-04-001
4
Male
Right angle




· Dimensions of Connector (Unit is mm)                                                     
Connector 
[image: ]

[image: ]

· General Information of Connector                                                          

Ambient Temperature:   -20℃ ~ +80℃                     Insulation Resistance:   ≥100MΩ             
Connector Body:        PBT, BLK/WHT                      Contact Resistance:     30mΩ Max.          
Connector Contacts:     Phosphor Bronze with gold plated      Shell:                 Stainless steel        
Fire Resistance：       UL94V-0                           Insert Force:           35N max.           


USB 2.0 Mini-B Male Molded Cable Assembly, Straight                             

[image: ][image: ]














· Dimensions of Cable Assembly (Unit is mm)                                                
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· General Information of Cable Assembly                                                    
Rated Current
1.0 A Max.
Rated Voltage
30V
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+60℃
Poles
5 Poles straight is available, right angle can be customized, refer to below SKU table
Cable
USB2.0 24-28AWG cable, PUR/PVC options

· SKU Table                                                                                
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-USB2.0MINBSTM-05-001
5
Male
Straight

T-USB2.0MINBRAM-05-001
5
Male
Right Angle




· Dimensions of Connector (Unit is mm)                                                     
Connector 
[image: ]



· General Information of Connector                                                          

Ambient Temperature:   -20℃ ~ +60℃                      Insulation Resistance:   ≥100MΩ             
Connector Body:        PBT, BLK/WHT                       Contact Resistance:     30mΩ Max.          
Connector Contacts:     Phosphor Bronze with gold plated       Shell:                 Stainless steel         
Fire Resistance：       UL94V-0                            Insert Force:           35N max.           






USB 2.0 Micro B Male Molded Cable Assembly, Straight                             

[image: ][image: ]














· Dimensions of Cable Assembly (Unit is mm)                                                            

[image: ]










· General Information of Cable Assembly                                                    
Rated Current
Signal (Pins 2,3,4): 1.0A Max., Power (Pins 1,5): 1.8 A
Rated Voltage
30V
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
5 Poles is available, refer to below SKU table
Cable
USB2.0 24-28AWG cable, PUR/PVC options

· SKU Table                                                                                
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-USB2.0MICBSTM-05-001
5
Male
Straight




· Dimensions of Connector (Unit is mm)                                                     
Connector 
[image: ]



· General Information of Connector                                                          

Ambient Temperature:   -20℃ ~ +80℃                      Insulation Resistance:   ≥100MΩ             
Connector Body:        PBT, BLK/WHT                      Contact Resistance:     50mΩ Max.          
Connector Contacts:     Phosphor Bronze with gold plated       Shell:                Stainless steel        
Fire resistance：        UL94V-0                           Insert Force:           35N max.           



USB 2.0 Micro B Male Molded Cable Assembly, right angle                             
[image: ][image: ]














· Dimensions of Cable Assembly (Unit is mm)                                                            
[image: ]












· General Information of Cable Assembly                                                    
Rated Current
Signal (Pins 2,3,4): 1.0A Max., Power (Pins 1,5): 1.8 A
Rated Voltage
30V
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+50℃
Poles
5 Poles is available, refer to below SKU table
Cable
USB2.0 24-28AWG cable ,PUR/PVC options

· SKU Table                                                                                
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-USB2.0MICBRAM-05-001
5
Male
Right angle




· Dimensions of Connector (Unit is mm)                                                     
Connector 
[image: ]










· General Information of Connector                                                          

Ambient Temperature:   -20℃ ~+80℃                      Insulation Resistance:   ≥100MΩ             
Connector Body:        PBT, BLK/WHT                      Contact Resistance:     50mΩ Max.          
Connector Contacts:     Phosphor Bronze with gold plated       Shell:                Stainless steel        
Fire resistance：        UL94V-0                           Insert Force:           35N max.           


USB 3.0 Type A Female Molded Cable Assembly 
[image: ] [image: ] 







· Dimensions of Cable Assembly (Unit is mm)                                                
[image: ]
















· SKU Table                                                                                        
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-USB3.0ARAF-09-001
9
Female
Right Angle

T-USB3.0ASTF-09-001
9
Female
Straight


· General Information of Cable Assembly                                                    
Transmission Speed
5Gbps(640MB/s)
Rated Voltage
30V
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
9 Poles right angle is available, straight can be customized ( Refer to SKU table）
Cable
PUR/PVC cable (28AWG) options


· Related Components (Unit is mm, refer to if it is without tolerance)                                                         Connector
[image: ]
[image: ]


· General Information of Connector                                                          
Ambient Temperature:   -20℃ ~ +80℃                     Insulation Resistance:   ≥100MΩ              
Connector Body:        PBT, Blue                          Contact Resistance:     50mΩ Max.           
Connector Contacts:     Copper Alloy with gold plated         Shell:                 Stainless steel         
Fire resistance：        UL94V-0                          Mating Force:          3.57KG max.           




USB 3.0 Type A Male Molded Cable Assembly, Straight                             

[image: ][image: ]













· Dimensions of Cable Assembly (Unit is mm, refer to if it is without tolerance)                                                            
[image: ]










· General Information of Cable Assembly                                                    
Transmission Speed
5Gbps(640MB/s)
Rated Voltage
30V
Insulation Resistance
≥100MΩ
Contact Resistance
≤5Ω
Operation Temperature
-20℃ ~+80℃
Poles
9 Poles straight are available, 
9 Poles right angle can be customized （Refer to below SKU table）
Cable
PUR/PVC cable (28AWG) options

· SKU Table                                                                                
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-USB3.0ASTM-09-001
9
Male
Straight

T-USB3.0ARAM-09-001
9
Male
Right Angle



· Dimensions of Connector (Unit is mm, refer to if it is without tolerance)                                                                 Connector 

[image: ]
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· General Information of Connector                                                          

Ambient Temperature:   -20℃ ~ +80℃                     Insulation Resistance:   ≥100MΩ             
Connector Body:        PBT, blue                          Contact Resistance:     50mΩ Max.          
Connector Contacts:     Phosphor Bronze with gold plated      Shell:                 Available             
Fire resistance：        UL94V-0                          Mating Force:          3.57KG max.          

USB 3.0 Micro-B Male Molded Cable Assembly, Straight                             

[image: ][image: ]













· Dimensions of Cable Assembly (mm, refer to if it is without tolerance)                                                           
[image: ]










· SKU Table                                                                                
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-USB3.0MICBSTM-10-001
10
Male
Straight


· General Information of Cable Assembly                                                    
Transmission Speed
5Gbps(640MB/s)
Rated Voltage
30V
Insulation Resistance
≥10MΩ
Contact Resistance
≤3Ω
Operation Temperature
-20℃ ~+80℃
Poles
10 Poles straight are available, Refer to below SKU table
Cable
PUR/PVC cable (28AWG) options


· Dimensions of Connector (Unit is mm, refer to if it is without tolerance)                                                                 [image: ]





· General Information of Connector                                                          

Ambient Temperature:   -20℃ ~ +80℃                     Insulation Resistance:   ≥100MΩ             
Connector Body:        PBT, black                         Contact Resistance:     50mΩ Max.           
Connector Contacts:     Phosphor Bronze with gold plated      Shell:                 Available             
Fire resistance：        UL94V-0                          Mating Force:          3.57KG max.          

Type C Male Molded Cable Assembly, Straight                             

 [image: ][image: ]













· Dimensions of Cable Assembly (Unit is mm, refer to if it is without tolerance)                                                           
[image: ]










· General Information of Cable Assembly                                                    
Transmission Speed
10Gbit (1000MB/s)
Rated Voltage
30V
Rated Current/Power delivery
5A Max. /Also provide the 100W (20V/5A) electric power
Insulation Resistance
≥10MΩ
Contact Resistance
≤3Ω
Operation Temperature
-20℃ ~+80℃
Poles
A12+B12 Poles straight and right angle are available, Refer to below SKU table
Cable
PUR/PVC cable (28-32AWG) options

· SKU Table                                                                                
SKU No.
Poles
Conn. Type
Overmoding Type
Remark
T-USB3.0TCSTM-24-001
24
Male
Straight

T-USB3.0TCRAM-24-001
24
Male
Right angle



· Dimensions of Connector (Unit is mm, refer to if it is without tolerance)                                                                  
[image: ]

Pinout definition of male
[image: ]



· General Information of Connector                                                          

Ambient Temperature:   -55℃ ~ +85℃                     Insulation Resistance:   ≥100MΩ             
Connector Body:        PBT, black                         Contact Resistance:     30mΩ Max.           
Connector Contacts:     Phosphor Bronze with gold plated      Life Cycles:            10K Times                
Fire resistance：        UL94V-0                          Mating/Pull Force:      3.57Kgf max./1.02Kgf Min.          



TOTEK INTERNATIONAL CORPORATION LTD                        Mail: cma@totekinternational.com  TEL:+86-769-81519919    
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